The enclosed Quick Tape version is a service for owners of an original license
whose original cassette or EPROM can no longer be read without errors. 
For vintage computing only, not for commercial use, no warranty!

This software is based on an older Quick Tape version with a PC-1500 header, 
developed and distributed with RWEtool 4 
by Ralf & Werner Eckstein, Fischerweg 15, Zirndorf 

There are extended versions with faster headers on cassettes in PC-WORK 
(distributed by RVS Datentechnik through Holtkötter Verlag, Hamburg) 
and as hardware extensions (EPROM, IWS, etc). 
see also http://www.pc-1500.info/2014/08/07/holtkotter-pc-software-rvs/

Quick-Tape with PC-1500 standard header, installation and use
-------------------------------------------------------------

1. This version Quicktape_C5 only works on a PC-1500(A) WITH CE-161 AND CE-150
                                                        ----        ---
2. Clear all and free memory space
   [Mode] Pro
   NEW 705

3. Use MC2Wav.cmd, see the manual (how)to make wav file from bin file
   Quicktape_C5.BIN and Quicktape_C5.CFG 
   Load binary programm with CLOAD M (Address &C5 included, Length 508)

4.  Use Rsv2Wav.cmd, see the manual (how)to make wav file from rsv file
    Quicktape_C5.RSV
    [Shift] [Mode] Reserve, Keys F1-F3 load with CLOAD

5. Use the RSV Keys

Set Z$ correctly FIRST and after NEW or have to use [BRK]
CE-161: Load address &00C5

Reserve Keys I
QSAVE	[F1] CALL &C9,Z$ Save BASIC  (Z$=prog.name)
QLOAD ?	[F2] CALL &CB	 Verify BASIC 
QLOAD	[F3] CALL &CA	 Load BASIC 

Reserve Keys II
QSAVE M	[F1] CALL &C7,Z$ Save machine code (A=start address, B=end, Z$=name)
QVERIFY [F2] CALL &C5	 Verify (Load) machine code
QLOAD M	[F3] CALL &C6	 Load machine code (A=start address)

Copyright/authors: Ralf & Werner Eckstein, 1984-1986
RVS Datentechnik, Holtkötter Hamburg, IWS (W. Speidel) 1985, 
ECPS Rainer Kratzer 1987
